**Section 10 11 16.13 (Section 10115) - Fixed Marker Boards**

PART 1 - GENERAL

* 1. Section Includes
     1. Fixed, glass, dry erase marker boards, and magnetic whiteboards.
  2. Scope
     1. Furnish glass panels, wall mounting hardware, and anchors as necessary.
  3. Submittals
     1. Comply with Section 01330 (01 33 00) – Submittal Procedures.
     2. Product Data: Submit manufacturer’s product data, including installation instructions.
     3. Samples: Submit manufacturer’s sample of marker boards.
     4. Cleaning Instructions: Submit manufacturer’s cleaning instructions.
     5. Warranty Documentation: Submit manufacturer’s standard warranty.
  4. Quality Assurance
     1. Manufacturer to have a minimum of 5 years experience producing glass marker boards.

1. PRODUCTS
   1. Acceptable Supplier
      1. MDC

400 High Grove Blvd

Glendale Heights, IL 60139

(800) 621-4006

[cs@mdcwall.com](mailto:cs@mdcwall.com)

* + 1. Substitutes: Substitutes are not acceptable.
  1. Glass Marker Boards
     1. Material: ¼” thick [clear] [low-iron] tempered safety glass
     2. Size
        1. As required per plans and specifications
     3. Finishes
        1. Back painted White with ceramic frit coating permanently fused during tempering
        2. Back painted Black with ceramic frit coating permanently fused during tempering
        3. Back painted Custom Color
     4. Mounting
        1. Provide “Z” clip style mounting brackets
           1. Z clip mounting to be tested for a minimum of 3 years for stability
        2. Provide stainless steel standoffs
        3. Provide appropriate anchors to mount on drywall, concrete, or other surface.
        4. Use only manufacturer approved and provided hardware
  2. Glass Magnetic Marker Boards
     1. Material: ¼” thick [clear] [low-iron] tempered safety glass
     2. Size
        1. As required per plans and specifications
     3. Finishes
        1. Back painted White with ceramic frit coating permanently fused during tempering
        2. Back painted Black with ceramic frit coating permanently fused during tempering
        3. Back painted Custom Color
     4. Backing
        1. Magnetic manufacturers standard magnetic backing
     5. Mounting
        1. Provide “Z” clip style mounting brackets
        2. Provide stainless steel standoffs
        3. Provide appropriate anchors to mount on drywall, concrete, or other surface.
        4. Use only manufacturer approved and provided hardware

1. EXECUTION
   1. Installation
      1. A qualified installer shall install glass dry erase boards.
      2. Install dry erase boards level, plumb, and at the height indicated
   2. Cleaning
      1. Clean marker boards promptly after installation in accordance with manufacturer’s instructions.
      2. Do not use harsh cleaning materials or methods that could damage surface.
   3. Warranty
      1. Lifetime on surface finish

END OF SECTION